  Tender No.: BHDC-BID-2026-078


INVITATION TO BID 
Subject: 750HP Workover Rig Service in the Missan and North-Central Iraq Areas
Tender No.: BHDC-BID-2026-078
Date: Sep 2nd, 2026
Dear Sirs,
CNPC Bohai Drilling Engineering Company Limited – Iraq Branch (hereinafter referred to as the “Tenderee”) is pleased to invite your esteemed company to submit a sealed Bid for the above-mentioned Tender.
Your Bid shall be prepared and submitted strictly in accordance with the following Invitation to Bid (ITB) documents:
           Section Ⅰ: Acknowledgment Form

           Section Ⅱ: Instructions to Bidders 

All costs incurred in the preparation and submission of the Bid shall be borne solely by the Bidder and shall not be reimbursed by the Tenderee under any circumstances. The Tenderee shall not be responsible for any loss and/or delay in the delivery of submitted proposals. The Tenderee reserves the right to reject any or all Bids or to accept the Bid of any Bidder(s) at its sole discretion without assigning any reason.
The Tender Documents shall be submitted by email. Any bidding samples shall be submitted in strict accordance with Clause 10, Part I of Section II of the ITB. Bidding related Email address:

Bidding Email Addresses: 

tender@bhdc-iraq.com
qin.jun@bhdc-iraq.com
zhang.sujie@bhdc-iraq.com
Please complete and return the Acknowledgment Form (Section I) by email to confirm your intention to participate within three (3) days upon receipt of this Invitation to Bid. 

IMPORTANT 
ALL BIDDERS MUST READ THE INSTRUCTIONS TO BIDDERS CAREFULLY AND SUBMIT THEIR PROPOSALS IN STRICT COMPLIANCE WITH THE REQUIREMENTS PROVIDED HEREIN.

FAILURE TO COMPLY MAY RESULT IN DISQUALIFICATION OF THE BID FROM FURTHER CONSIDERATION.
Authorized Signature & Stamp: ________________________________
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SECTION I    ACKNOWLEDGEMENT FORM
To:  CNPC Bohai Drilling Engineering Company Limited- Iraq Branch

E-mail: tender@bhdc-iraq.com; qin.jun@bhdc-iraq.com;zhang.sujie@bhdc-iraq.com
Tender No.: BHDC-BID-2026-078

Note: The Bidder is required to indicate its intention to participate in this Tender by completing and returning this form within three (3) calendar days from the issuance date of the Invitation to Bid documents (“ITB Documents”).

We hereby acknowledge receipt of your ITB Documents for the above-mentioned services.

A) Intention to Submit a Bid

We hereby confirm our intention to submit a complete, compliant, and authentic Bid by the date and time specified in the Invitation to Bid Letter. We further confirm that we have received the full set of ITB Documents with no missing or incorrect pages.
Contact person responsible for this Tender:

Name…………………………………         Designation………………………………

Telephone No ………………………           Extension…………………………………

Fax No………………………………           E-mail ……………………………………


B) Decline to Participate

Please be advised that we will not be participating in this Tender for the following reason(s):
………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………………

ITB Documents to be returned by (if applicable):…………………………………………………….

*Please delete either Section A or Section B as applicable.

Acknowledgement:

Signature: 
………………………………………

Name: 
……………………………………………………. ………… 

Designation……………………………………………………………

Date:
……………………………………………………. …………

Company Address and Stamp: 
………………………………………

SECTION II    INSTRUCTIONS TO BIDDER

PART I  GENERAL INSTRUCTIONS TO BIDDERS

1. GENERAL DESCRIPTION

1.1 CNPC Bohai Drilling Engineering Company Limited – Iraq Branch (hereinafter referred to as the “Tenderee”) invites bids for the provision of 750HP Workover Rig Service in the Missan and North-Central Iraq Areas. The detailed technical requirements and scope of services are specified in the Technical Proposal (Part II of Section II) of the Invitation to Bid (ITB) 

1.2 The Tenderee shall enter into a contract with the successful Bidder. The prices quoted in the Bid shall remain fixed and valid for the entire duration of the contract and shall not be subject to adjustment unless otherwise expressly stated in the contract.

2. COMPLIANCE WITH ITB 

2.1 The Bidder shall submit a base Bid Proposal that fully complies with all requirements set forth in this Invitation to Bid (ITB). Submission of a fully compliant Bid is a mandatory prerequisite. Any clarifications, deviations, exceptions, exclusions, conditions, variations, assumptions, reservations, or rejections of the terms and conditions included in the Bid shall be deemed deviations from the ITB. Any Bid containing such deviations may be disqualified and rejected by the Tenderee at its sole discretion.
2.2 The Bidder is advised to respond to the ITB using clear, definitive, and positive statements. Any vague, conditional, or ambiguous responses shall be deemed non-compliant with, or deviations from, this ITB.
2.3 Notwithstanding the above, the Bidder may list any departures from the ITB requirements strictly in ATTACHMENT 2-C (Deviations / Exceptions Form). The Tenderee shall not recognize and shall fully disregard any deviation(s) or exception(s) not stated in the designated Technical Proposal Forms, including any such statements mentioned elsewhere in the Technical Proposal and/or Commercial Proposal. The Tenderee shall bear no obligation of any kind with respect to any listed deviations or exceptions.

3. DEVIATIONS/EXCEPTIONS BY BIDDER

All Deviation(s) / Exception(s) without any cost impact shall be listed in ATTACHMENT 2-C and included as part of the Technical Proposal. 

All Deviation(s) / Exception(s) involving any cost impact shall be listed in ATTACHMENT 3-B and included as part of the Commercial Proposal.

4. ITB ACKNOWLEDGEMENT

(Reference: Section I – Acknowledgment Form)

4.1 Completeness of ITB Documents

The Bidder shall carefully examine the contents of the Invitation to Bid (ITB) Documents to ensure that there are no omissions, inconsistencies, or discrepancies. The Bidder shall promptly notify the Tenderee in writing of any omissions, discrepancies, or uncertainties identified in the ITB Documents, including any doubt as to the precise meaning of any item, word, figure, term, or requirement.
4.2 Intention to Bid

The Bidder shall complete the Acknowledgment Form (Section I) and submit it to the Tenderee within two (2) calendar days from the issuance date of the ITB Documents to confirm its intention to participate in the Tender.

The Bidder is also required to confirm its official company name and registered address and to designate a duly authorized representative to whom all communications from the Tenderee shall be directed.

4.3 Decline to Bid

Should the Bidder decide not to submit a Bid, the Bidder shall state the reason(s) for declining participation in the Acknowledgment Form and return the completed form to the Tenderee by email.

5. INTERPRETATION OF ITB

5.1 All requests for clarification, interpretation, or explanation of any part of the Invitation to Bid (ITB) Documents shall be submitted in writing by email only to the following addresses:
tender@bhdc-iraq.com
qin.jun@bhdc-iraq.com
zhang.sujie@bhdc-iraq.com

5.2 In the event that the Bidder identifies any discrepancies, errors, ambiguities, or omissions in any part of the ITB Documents, the Bidder shall immediately request clarification or interpretation from the Tenderee in accordance with Clause 5.1. 

6. EQUALITY OF SUPPLY OF INFORMATION

Copies of all requests for interpretation received from Bidders and the corresponding written responses issued by the Tenderee shall be distributed to all Bidders to ensure that all parties are provided with the same information and that the bidding process remains fair, transparent, and comparable.

7. ORAL INTERPRETATION
The Tenderee shall not be bound by any oral statements, explanations, or interpretations of the ITB made by the Tenderee or any of its representatives. Only written interpretations formally issued by the Tenderee in accordance with the procedures stipulated in this ITB shall be deemed official and binding upon the Tenderee.

8. IMPLIED AGREEMENT
Where the Bidder’s Bid does not contain any expressly stated deviations or exceptions submitted in accordance with Clause 2 of this ITB, the Bidder shall be deemed to have fully accepted all terms, conditions, and requirements of the ITB without reservation.

9. SUBMISSION OF BID

9.1 The Bidder shall submit its Tender in digital format by email only. All Tender Documents shall be provided as soft copies in Adobe PDF (*.pdf) format, together with editable digital files. 

Each submission package shall be clearly marked as follows:

“CONFIDENTIAL-TECHNICAL BID FOR TENDER NO. BHDC-BID-2026-078”

“CONFIDENTIAL-COMMERCIAL BID FOR TENDER NO. BHDC-BID-2026-078”

Technical Bid and Commercial Bid packages shall be submitted via email:

Email:
 tender@bhdc-iraq.com; 
zhang.sujie@bhdc-iraq.com;
qin.jun@bhdc-iraq.com
9.2 The Bidder’s registered company name shall be inserted at the footer of every page of both the Technical Proposal and the Commercial Proposal.

9.3 Full responsibility for ensuring the timely delivery of the Bid to the correct email addresses within the specified deadline rests solely with the Bidder. The Tenderee shall not accept any late submissions and shall bear no liability whatsoever for any failure, delay, or non-receipt of any Bid submission.
10. GENERAL REQUIREMENT

10.1 The language of all documents and communications relating to this Bid shall be English.
10.2 The Bidder shall ensure that all prices, calculations, data, and other details contained in the Bid are accurate and complete at the time of submission. The Tenderee shall not accept or consider any amendment, correction, or revision arising from arithmetical or clerical errors after the Bid Closing Date.

10.3 All costs incurred in connection with the preparation and submission of the Bid, including but not limited to any clarification requests, discussions, communications, presentations, meetings, or site visits, shall be borne solely by the Bidder, regardless of whether a Contract is awarded or executed.

11. BID PRICE

All prices shall be quoted in United States Dollars (USD) only. Bids submitted in any other currency shall not be accepted.
12. LICENSING

The Bidder shall obtain and submit copies of all required consents, permits, licenses, approvals, authorizations, certifications, registrations, and/or waivers necessary for the performance of the Services in accordance with applicable laws and regulations.

13. BID CLOSING DATE

The Bidder shall ensure that both the Bid documents and any required samples are delivered to the designated addresses specified in Clause 9 and Clause 10 of this ITB on or before the Bid Closing Date and time. Any Bid or sample received after the stipulated deadline shall be rejected unopened and shall not be considered.

Bid Closing Date and time:

Technical Bid and Commercial Bid:
 17:00 pm, Iraq time, on Sep 9th, 2026. 
14. CLARIFICATIONS

The Tenderee reserves the right to request clarifications from any Bidder after the submission of Bids.

Bidders submitting a Bid that fails to comply with the instructions set forth in this ITB—including but not limited to unclear or ambiguous responses, internal inconsistencies, deviations from the ITB, or submission after the Bid Closing Date—do so at their own risk. Such Bids may be rejected by the Tenderee without further opportunity for amendment or correction.

15. CONSIDERATION OF BID

15.1 The Tenderee reserves the right to request any additional information it may deem necessary to properly evaluate a Bid. Such requests may include, but are not limited to, a detailed breakdown or supplemental explanation of any prices, rates, or percentages proposed in the Bid.
15.2 All Bids submitted shall become the property of the Tenderee. No part of any Bid will be returned to the Bidder under any circumstances.

16. ACCEPTANCE OF BID

16.1 The Tenderee reserves the right to reject any or all Bids received, or to accept any Bid which, in the sole judgment of the Tenderee, is most advantageous. The Tenderee may accept or reject all or part(s) of any Bid at its sole discretion and shall have no obligation to provide reasons for its decision.

16.2 The successful Bidder shall be required to enter into a formal contract with the Tenderee. Such contract shall be on the same terms and subject to the same conditions as contained in the ITB Documents, except as may be amended by any clarifications issued during or prior to the evaluation of the Bid.

16.3 No Bid shall be deemed accepted by the Tenderee unless and until either: A Contract is duly executed by both parties, or The Tenderee issues a Letter of Intent to Award to the successful Bidder, duly signed by an authorized representative of the Tenderee.
17. REQUEST FOR FURTHER INFORMATION BY BIDDER

17.1 Any additional information or clarification required by the Bidder to complete its Bid, or any interpretation thereof, must be requested in writing or by facsimile, sent to the addresses specified in this ITB.

17.2 All such requests must be submitted no later than three (3) calendar days prior to the Bid Closing Date.

17.3 Except as expressly provided in this ITB, the Bidder is not permitted to contact or communicate with any member of the Tenderee’s staff, or any personnel of consultant companies engaged by the Tenderee for the preparation of the ITB Documents, regarding any matter relating to this Bid. Unscheduled or uninvited visits to the Tenderee’s offices for discussions concerning the ITB Documents are strictly prohibited.

18. MODIFICATION BY TENDEREE

18.1 The Tenderee reserves the right to modify the ITB Documents after issuance to the Bidders. Any modification made by the Tenderee shall be communicated to all Bidders no later than seven (7) calendar days prior to the Bid Closing Date.
All modifications shall be issued in the form of Invitation to Bid Supplements (e.g., Notice-to-Bidders and/or Addenda) and shall be deemed to form an integral part of the ITB Documents. In the event of any conflict between the original ITB Documents and subsequent addenda, the latest addendum in time shall prevail. The Bidder shall include in its Bid the cost of all work and requirements contained in the issued addenda.

18.2 The Tenderee further reserves the right to issue clarifications or modifications to the ITB Documents during the Bid evaluation period, if deemed necessary.

19. CONFIDENTIALITY OF BID

By submitting a Bid, the Bidder warrants and undertakes that:

19.1 All documents provided by the Tenderee shall be treated as confidential and used solely for the purpose of preparing the Bid. Such documents shall not be duplicated, disclosed, or used for any other purpose except to the extent required for the preparation of the Bid in response to this Invitation to Bid.
19.2 All prices and other terms contained in the Bid have been determined independently, without consultation, communication, agreement, or understanding with any other bidder or competitor for the purpose of restricting competition.
19.3 Unless required by applicable law, the prices and other commercial information quoted in the Bid have not been, and shall not be, disclosed, directly or indirectly, to any other bidder or competitor.
19.4 The Bidder has not and will not attempt to induce any other person or company to submit or refrain from submitting a Bid with the purpose of restricting competition. The Bidder affirms adherence to the highest standards of business ethics, including the establishment of precautions to prevent its officers, employees, or agents from offering, receiving, or soliciting substantial gifts, entertainment, payments, loans, or other considerations that could improperly influence any person in connection with this Invitation to Bid.
20. VALIDITY OF BID

The Bid submitted by the Bidder shall be binding, irrevocable, and valid for a period of sixty (60) calendar days from the Bid Closing Date. Any withdrawal, modification, or alteration of any statement, term, condition, or price in the Bid during this validity period shall render the Bid automatically rejected by the Tenderee.
PART II TECHNICAL PROPOSAL – CONTENTS AND REQUIREMENTS

1. SCOPE OF TECHNICAL PROPOSAL
a) The Bidder shall supply one 750HP workover rig, complete with all associated equipment and ancillary services, to the Company for operations within the Missan and North-Central Iraq regions.
b) The Bidder shall also undertake full mobilization of the equipment, covering transportation, customs clearance, and on-site delivery Company's designated the work sites. Any and all legal risks arising from the customs transit or transshipment of the equipment shall not be attributable to the Company.
c) The Contract shall have an initial firm term of two (2) years, with a unilateral option held by the Company to extend for one (1) additional year at its sole discretion, provided, however, that such extension shall be conditional upon the renewal of the master workover service contract between the Company and the Principal. The Company shall exercise such option by giving the other Party at least thirty (30) days' prior written notice before the expiry of the initial term.
d) Delivery Schedule: Upon the effectiveness of this Agreement, bidder shall deliver the Equipment to the Delivery Location within thirty (30) days after the effective date of this Agreement. In the event of any delay beyond the said thirty-day period, the Company may, at its sole discretion, terminate this Agreement by written notice to the Contractor.
e) Delivery Location: The Equipment shall be transported and delivered to the Company‑specified well site (hereinafter referred to as the “Delivery Location”).
f) After the equipment arrives at the delivery location, Company and Bidder shall jointly conduct an arrival inspection, which includes, but is not limited to, the counting of equipment and accessory quantities, as well as the performance acceptance test of the equipment in operation. Upon successful completion of such inspection, an acceptance report shall be prepared, and the authorized representatives of both parties shall sign the said report to confirm the handover facts and the current condition of the equipment. Upon completion of the aforesaid inspection and the signing of the acceptance report, the equipment shall be deemed to have passed the acceptance inspection. Equipment Acceptance Key Checklist as follow:
	Item
	Key Indicator
	Acceptance Criteria
	Result
	Remarks

	I. Visual & Structural

	1
	Structural Deformation
	Mast/substructure/chassis deformation ≤ ±5mm/m
	☐ Pass ☐ Fail
	

	2
	Structural Cracks
	No visible cracks on critical components
	☐ Pass ☐ Fail
	

	3
	Corrosion Depth
	Local corrosion ≤ 10% of original thickness
	☐ Pass ☐ Fail
	

	4
	Component Completeness
	Matches configuration list, no missing parts
	☐ Pass ☐ Fail
	

	II. Power & Transmission

	5
	Engine Start-up
	Start-up time ≤ 15 seconds
	☐ Pass ☐ Fail
	

	6
	Engine Operation
	No knocking/rubbing/leakage sounds
	☐ Pass ☐ Fail
	

	7
	Engine Load Test
	Stable output, no power drop/black smoke
	☐ Pass ☐ Fail
	

	8
	Driveshaft Runout
	Radial runout ≤ 0.8mm
	☐ Pass ☐ Fail
	

	9
	Gear Shifting
	Smooth, no sticking/abnormal noise
	☐ Pass ☐ Fail
	

	III. Hoisting & Hydraulic

	10
	Wireline Condition
	No broken wires, diameter wear ≤ 10% of original
	☐ Pass ☐ Fail
	

	11
	Brake Slippage (Full Load)
	Slippage distance after braking ≤ 50mm
	☐ Pass ☐ Fail
	

	12
	Hydraulic Sealing
	No oil leaks at hoses/fittings
	☐ Pass ☐ Fail
	

	13
	Hydraulic Pressure Stability
	Fluctuation ≤ ±5% of set value
	☐ Pass ☐ Fail
	

	14
	Cylinder Operation
	Smooth extension/retraction, no creeping/juddering
	☐ Pass ☐ Fail
	

	IV. Electrical & Safety

	15
	Insulation Resistance
	≥ 0.5MΩ
	☐ Pass ☐ Fail
	

	16
	Ground Resistance
	≤ 4Ω
	☐ Pass ☐ Fail
	

	17
	Emergency Stop (E-stop)
	Immediate stop upon pressing
	☐ Pass ☐ Fail
	

	18
	Brake Pad Thickness
	≥ 1/3 of original thickness
	☐ Pass ☐ Fail
	

	19
	Full-load Braking Force
	Prompt stop without slippage under full load
	☐ Pass ☐ Fail
	

	20
	Guardrails
	Height ≥ 1.05m, securely fixed
	☐ Pass ☐ Fail
	

	V. Documentation

	21
	Factory Certificate of Conformity
	Original copy available
	☐ Pass ☐ Fail
	

	22
	Operation Manual & Maintenance Records
	Complete
	☐ Pass ☐ Fail
	


i) Responsibilities Matrix
	Item
	Designation
	Provided by Company
	Paid

by Company
	Provided by

Bidder
	Paid by 

Bidder

	1
	Mobilization (including transportation, loading/unloading, and transit insurance)
	
	√
	√
	

	2
	Demobilization (including dismantling, loading, and return transportation)
	
	
	√
	√

	3
	Provision of XJ750 workover rig and all ancillary equipment (including mast, crown block, traveling block, hook, swivel, rotary table, drawworks, mud pumps, etc.) conforming to technical specifications
	
	√
	√
	

	4
	Registration, licensing, and vehicle registration certificates (license plates/registration books) for temporarily imported vehicles and equipment provided by Bidder, the cost of which is included in the Mobilization Fee
	
	√
	√
	

	5
	Provision of technical documentation, drawings, and operation manuals for the equipment
	
	
	√
	√

	6
	Routine maintenance, servicing, repair, and spare parts replacement during the equipment usage period
	√
	√
	
	


The Bidder shall submit a Technical Proposal, which clearly addresses all non-commercial aspects of the Bidder’s submission.

The Technical Proposal shall be prepared in accordance with the following Table of Contents and the requirements set forth in the preceding sections:

Part 1) Bidder Profile and Organization

Part 2) Experience (ATTACHMENT 2-A)

Part 3) Equipment Proposal (ATTACHMENT 2-B)
Part 4) Summary of Deviations/Exceptions (ATTACHMENT 2-C)  

Part 5) Litigation (ATTACHMENT 2-D)

Part 6) Confidentiality and Secrecy (ATTACHMENT 2-E)         

Part 7) Other matters at Bidder’s discretion  

The Technical Proposal shall be comprehensive, well-organized, and presented in a professional manner, ensuring that all requested information is clearly provided. 

2. DETAILS REQUIREMENT

2.1 Bidder Profile and Organization

Bidder is required to provide information about the company which shall include:

a) Company Profile – Overview of the company, organizational structure, and key personnel.
b) Company Registration Certificate or Business License issued by Iraqi Ministry of trade 

c) Tax Registration Certificate and Tax Card issued by Iraqi Ministry of Finance
d) Official Bank Certificate for Opening the Corporate Account 

e) the Legal Representative’s National ID Card and Passport.
f) Power of Attorney or Authorization Letter

g) Other Qualification Documents

2.2 Experience 
The Bidder's experience shall be completed and provided in accordance with the requirements set forth in ATTACHMENT 2-A EXPERIENCE.
2.3 Equipment Proposal
The Bidder's Equipment Proposal shall be completed and provided in accordance with the requirements set forth in ATTACHMENT 2-B EQUIPMENT PROPOSAL.

2.4 Summary of Deviations/ Exceptions

The Bidder shall clearly detail all proposed deviations or exceptions from the requirements of this ITB. 

Such deviations or exceptions must be summarized using the Summary of Deviations/Exceptions Form (ATTACHMENT 2-C). Any deviations or exceptions not included in ATTACHMENT 2-C shall not be considered by the Tenderee. 
Notwithstanding the submission of any deviations or exceptions, the Tenderee shall not be bound or obligated to accept any such deviations or exceptions, and they shall have no effect on the rights or obligations of the Tenderee.

2.5 Business Standards

All Bidders shall be afforded an equal opportunity to secure a contract. The offering or receipt of gifts, entertainment, payments, loans, or any other favors with the intention of influencing placement on the Bidder’s list, obtaining a contract or purchase order, or receiving preferential treatment under a contract or purchase order is strictly prohibited.

It is the policy of Tenderee that, should any Bidder, vendor, or subBidder be found to have offered or provided such gratuities to secure a contract, purchase order, or favorable treatment, all parties involved shall be disqualified from further consideration in the bidding process. In addition, Tenderee reserves the right to pursue all remedies available under applicable law and the terms of the relevant CONTRACT or Purchase Order, including, without limitation, termination for default.

Bidders are specifically directed to review and comply with the articles of the CONTRACT or Purchase Order that govern legal obligations and consequences of default.

2.6 Litigation

The Bidder shall disclose whether it is currently involved, or has been involved in the past five (5) years, in any litigation, arbitration, or administrative proceedings. If so, the Bidder shall provide full details of such proceedings using the format specified in ATTACHMENT 2-D.

2.7 Confidentiality and Secrecy

The Bidder shall treat all ITB documents, information, and supporting materials as strictly confidential. The Bidder shall not disclose any such information to third parties without the prior written consent of Tenderee. Compliance with this requirement shall be formally acknowledged by executing the form provided in ATTACHMENT 2-E.

2.8 Other Matters at Bidder's Discretion

The Bidder may include any additional non-commercial information or disclosures that it believes will assist Tenderee in fully evaluating or understanding the Bidder’s proposal. Such information should be clearly presented and relevant to the proposal’s evaluation.

All documents and information provided by the Bidder must be true, accurate, and valid. Any Bid containing false, misleading, or fraudulent documents or information shall be disqualified and rejected by Tenderee.

PART III  COMMERCIAL PROPOSAL-CONTENTS AND REQUIREMENTS

1. SCOPE OF COMMERICIAL PROPOSAL

The Bidder shall submit a complete and clearly presented Commercial Proposal. The proposal shall be prepared in accordance with the Commercial Proposal Form (ATTACHMENT 3-A)           
2. DETAILED REQUIREMENTS

2.1 Currency

All prices must be quoted exclusively in U.S. Dollars (USD). Quotations in any other currency will not be accepted.

2.2 Quotation Form

Should the Bidder propose any deviations or exceptions that impact the pricing, such deviations/exceptions must be clearly listed in ATTACHMENT 3-B (Summary of Deviations/Exceptions). 

Bidders are advised to ensure that all commercial information is accurate, complete, and consistent with the technical proposal and any other bid documents.
(In Bidder's Letterhead)
ATTACHMENT 1 TECHNICAL CLARIFICATION FORM

Bidder shall list all clarification questions to this INVITATION TO BID
	ITB SECTION

(WITH PAGE NOS.)
	SUBJECT
	BIDDER'S QUESTION
	COMPANY’S RESPONSE

	
	
	
	

	
	
	
	


 (In Bidder's Letterhead)

ATTACHMENT 2-B EXPERIENCE 

	Year
	Name and country
	Value of Contract
	Address of Service

 (give also fax number or Email)
	Reference

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


ATTACHMENT 2-B EQUIPMENT PROPOSAL
	NO
	COMPANY’S REQUIREMENTS AND SPECIFICATIONS
	BIDDER’S PROPOSED SPECIFICATIONS

	1
	Work over Rig – General specification
	

	
	a. Rig Name/Rig type: 

b. Rig Owner and Rig Manager
c. Rig current status (Place; Cold stacking, hot stacking or working, etc.)
d. Year/date and Place manufactured
NOTE: the rig age must be no more than 15 years

e. Manufacturer:

f. Truck-mounted (other type is not acceptable)

g. Capacity: Minimum Capacity 650 HP. 

h. Rated working depth by using 3-1/2” DP (13.3 ppf), 2-3/8” DP(6.65ppf) etc.  respectively.

i. Substructure clear height vs height of BOPs including bell nipple (The bottom of tubing head flange is level with ground
j. Last overhaul year and date if have

k. Estimated Fuel Consumption Per Day (m3/day)

l. Rig layout: The dimension must be suitable for the rig site and could ensure rig equipment and vehicles move out and in smoothly, bidder is required to provide the dimension and diagram of its rig layout.

m. Delivery time: Must be no more than three months (90 days) since the mobilization order is effective.
n. The rig shall be diesel engine driven and equipped with heavy duty cooling systems. All diesel engines will be fitted with an emergency stop function.
The rig year/date of made, type, capacity and delivery time must meet the minimum requirements, otherwise bidder will be directly disqualified.

	

	2
	HOISTING EQUIPMENT 
	

	2.1
	Derrick/mast 

a. Manufacturer and model:

b. Type: Preferably telescoping type, double. 

c. Maximum Load capacity: shall be 150 MT as a minimum and be compatible to draw works with drill string racked in mast.

d. Dimension (when telescope out):

e. Year/date of Made: 

f. Height of monkey board (Measured from rig floor upward):

g. Last overhaul date if have:

h. Auxiliary Equipment: Monkey board for racking drill string stand.

Bidder failed to meet the minimum requirement will be directly disqualified.
	

	2.2
	SUBSTRUCTURE

a. Manufacturer and Model

b. Year/date of made: 
c. Latest inspection year and date:

d. Maximum static load capacity:150 MT as a minimum with DP or tubing stands racked in derrick.
e. Rig floor height and Clear height (From bottom of rotary table to ground) vs height of BOP stacks (including drilling spool+ bell nipple+annular+2 rams+ adapter)

Bidder failed to meet the minimum requirement will be directly disqualified.
	

	2.3
	DRUM DRAWWORKS 
a. Manufacturer and Model

b. Year/date of made: 
c. Type – Please Specify

d. Drive - 

e. Rated Input HP (Continuous) 

f. Type of brake and cooling system (COMPANY prefer would be a braking system that can safely handle workloads to full rig capacity without auxiliary brake back up)

g. Crown Block & Floor Protection device - (crown - floor saver)

h. Power available to draw works

i. Lift Capacity for the followings: 

1. At 8 lines                       ____ MT

2. At 6 lines                       ____ MT

3. At 4 lines                       ____ MT

j. Auxiliary Brake – Electric preferred or Hydromantic auxiliary brake with dump valve assembly c/w pneumatic foot-controlled actuator, & spare over running clutch assembly if required

k. Auxiliary brake Independent Cooling System – independent treated brake water system with after-coolers and pump

l. Draw works main & swab line drums equipped with “Lebus” type wear and kick back plates

m. Draw works main drum equipped with left or right hand “Lebus” type grooving, state “lay” of grooving and confirm line matches is size & lay 

COMPANY requires that the Draw works is either electrically driven (SCR) or be driven by an Allison type automatic transmission having no less than 6 forward gears and 1 reverse gear. Brake should preferably be twin disk electric with automatic speed control. Flange type brake rims should be equipped with water circulating cooling system.

Bidder failed to meet the minimum requirement will be directly disqualified.
	

	2.4
	CROWN BLOCK 

a. Make and Model:

b. Year/date of made: 

c. Maximum static load –150 MTs as a minimum

d. Number of Sheaves:

e. API Line size: 1-1/8”

f. Diameter (inch)：

g. Must be able to string back from 8 to 6 to 4 lines

h. Supply daily ton mile work schedule specifically designed for rig crown & traveling block assembly as per API line suppliers’ specifications.

i. Crown Sheave Cluster: Compatible to mast loads rating with the drilling line size.

Bidder failed to meet the minimum requirement will be directly disqualified.
	

	2.5
	Travelling block 

a. Make and Model:

b. Year/date of Made: 

c. Maximum static load –150 MT as a minimum

d. Number of Sheaves:

e. API Line size: 1-1/8”

f. Diameter (inch)

g. Must be able to string back from 8 to 6 to 4 lines

Bidder failed to meet the minimum requirement will be directly disqualified.
	

	2.6
	HOOK
a. Manufacturer

b. Year/date of Made:                                      

c. Model:

d. Maximum static hook load: 150 MT as a minimum

e. Must be equipped with minimum 3 position locking mechanism and compatible to or integral to traveling block.

f. Must be unlockable for free rotation under full load

Bidder failed to meet the minimum requirement will be directly disqualified.
	

	2.7
	CARRIER / DRAWWORKS PRIME MOVER

a. Manufacturer

b. Model

c. Year/date of Made: 

d. Engine Horsepower: shall be sufficient for operating the draw works.

e. Positive sealing air intake shut down

f. Spark arrestors fitted to exhaust system

g. Digital electric control system (optional, but recommended)

h. Sufficient radiator after cooler, coolant capacity to insure continuous operating capability in minimum +50°C temperature.

i. Equipped with auxiliary start, stop switches and normal operating gauge array at driller’s console.

COMPANY preference is a durable heavy duty diesel engine, electronically controlled to insure efficient fuel consumption with minimum emissions. 

Bidder failed to meet the minimum requirement will be directly disqualified.
	CARRIER / DRAWWORKS PRIME MOVER


	2.8
	LINKS

Forged and must be of sufficient length to accommodate double plug head below or back off swivel, maximum static load: 150 MT as a minimum,

a. Manufacturer

b. Model

c. Year/date of made:

d. Size (in)

e. Length (ft) minimum 9 ft

f. Maximum static load: 150 MT as a minimum

g. Quantities available (set):

Bidder failed to meet the minimum requirement will be directly disqualified.
	

	2.9
	DRILLING LINE (minimum specifications API 6X19 IWRC EIPS)

a. Size: must match to traveling block.

b. Type

c. API rating
	

	2.10
	DEADLINE ANCHOR (compression load cell type recommended)

a. Manufacturer

b. Model

c. Line size

d. Positioned in clearly lit and freely accessible area. 
	

	2.11
	Data Acquisition
A digital and graph or equivalent type equipment is required to monitor and record digitally the following information: Block height; Pump rate; pump pressure; hook load; trip tank level; rotary torque from power swivel or rotary table.

a. Manufacturer

b. Model
	

	3
	RIG FLOOR EQUIPMENT
	

	3.1
	Rotary table

a. Maximum Load Capacity: Compatible to mast and substructure (150 MT as a minimum)

b. Torque capacity: Compatible to depth rating
c. Torque indicator equipped
d. Size: Minimum 17.5 in

e. Year/date of made: 

Auxiliary equipment: Pin type drive locking master bushing, complete range of split inserts, lockable Kelly bushing with eccentric roller pin system.
	

	3.2
	CLOSED HEAD HYDRAULIC TUBING & LIGHT DRILL PIPE TONGS WITH DOUBLE ACTING JAWS AND PNEUMATIC OR HYDRAULIC BACK UP

a. Suitable for 2-3/8” – 5-1/2” tubular body.
b. Double acting jaws 2-3/8’’ - 5-1/2’’

c. Pneumatic or hydraulic back up 2-3/8’’ - 5-1/2’’

d. Easy read torque gauge & scale English, either metric or imperial

e. Solid, hinged, adjustable tong back up arm specifically designed to handle maximum reactive torque of power tong 

f. Tables as required compatible to jaws size range

g. Year/date of made:
	

	3.3
	BREAK OUT RAMS

a. Hydraulic minimum 4’ stroke

b. Automatic return

c. Mounted in mast

d. Minimum 12,000 ft*lbs single line pull

e. Adjustable line pulls pressure control device and gauge on operators control panel
	

	3.4
	CENTRE LATCH DRILL PIPE ELEVATORS

a. Qty: 1 set available for each size

b. Rated static load: 150 MT as a minimum

c. Center latch for 3-1/2” & 2-3/8’’, 18-degree DP

d. Year/date of made: 
	

	3.5
	CENTRE LATCH TUBING ELEVATORS 
a. Qty: 1 set available for each size

b. Rated static load: 120 MT as a minimum

c. For 3-1/2” EUE &VAM TOP, 2-7/8” EUE tubing 

d. Year/date of made: 
	

	3.9
	SAFETY CLAMPS

a. 2 complete set for small diameter range tubulars 2-7/8” through 4-1/2” minimum equivalency to Baash Ross type “T”

b. 2 complete set for larger diameter range tubulars 3-3/4” through 5-1/2” minimum equivalency to Baash Ross type “C”
c. Year/date of made:
	

	3.10
	WEIGHT INDICATOR 

Anchor or line sensor type

a. Manufacturer

b. Model

c. Gauge face plates for 4-, 6- & 8-line string ups

d. Latest calibration year and date:

Capable of record hook load with chart 24 hours a day.
	

	4
	ELECTRICAL POWER GENERATORS
	

	
	Must be equipped two sets of 350KW generators. BIDDER must supply manufacturer and “as built” wiring diagrams for all electrical equipment and installations, showing. All electrical equipment must be certified intrinsically safe and approved for use in a hazardous gaseous area, as per COMPANY approved governing body.

Bidder failed to meet the minimum requirement will be directly disqualified.
	

	4.1
	GENERATOR SETS 

a. minimum 1 matching 350 KW for rig site and camp site for sufficient power 

b. minimum 1 back-up with sufficient capacity to meet rig and camp requirements 

The generators shall be international brand, such as “Caterpillar” “Cummins”, “Volvo”, "Perkins" etc.,
	

	4.2
	SYCHRONIZING SWITCH GEAR

Electrical switch gear and breaker paneling must be equipped with minimum of 2 spare plug receptacles to facilitate hook of operator accommodations etc. Able to supply 3 phase power, capable of power 50Hz 220vlt. A complete set of as built drawings showing ratings and service of all electrical installations and related systems must be supplied to COMPANY for review and acceptance. All electrical supply and installations for rig package, including supporting camp must be safe for use hazardous area.
	

	4.3
	FUEL TANKS

Rig equipped with fuel storage capacity for 20 days operation as a minimum
	

	5
	TUBULARS
	

	5.1
	CROSSOVER SUBS

Supply complete range of API crossover subs for all BIDDER’s tubulars & related equipment as well as COMPANY’s normal thread sizes. 

Minimum length of each sub - 2 feet

Qty: Min. 1 each

Bidder shall provide the following cross overs.
3-1/2” EUE B X 3-1/2” Vam top P ,
3-1/2” Vam top B X 3-1/2” EUE P
3-1/2” EUE B X 2-7/8 “EUE P
3-1/2” Vam top B X 2-7/8” EUE P
3-1/2” EUE B X NC38 P 
a. Other type deems necessary as contractor consideration
b. Year/date of made: 
	

	6
	TUBULAR & TUBING RUNNING EQUIPMENT
	

	6.1
	MANUAL DRILL PIPE, TUBING SLIPS 

a. 1 set each 4-1/2”, tubing slips 

 
	

	7
	MUD CIRCULATING SYSTEMS
	

	7.1
	MUD PUMP

All pumps must be single acting Triplex plunger pump with automatic transmission: 
2 sets of 600 HP as a minimum.

a. Working pressure: 5000psi. 

b.  Pump must be rated for 5K and shall be > 8 bbls/minute
c.  Plunger sizes available: 

d.  Manufacturer:

e.  Model:

f. Type of pump: must be automatic transmission plunger type.

g. Rated horse power: Minimum 600HP.

h. Year/date of made of each set: 

i. Qty: 2 sets * 600HP
j. Transmission type:

k. Current place:

l.  Last overhaul year and date if have:

m.  Equipped with positive sealing, automatic shutdown control, temperature gauges pump pressure gauge, stop switches, and normal gauge array at operator station.

n.  Equipped with 4” x 5” hydraulic or electrically driven charge pump.

o.  Adequately illuminated for safe 24hr operation

p.  Transport System: Carrier or oilfield bed loadable skid mounted.
Bidder failed to meet the minimum requirement will be directly disqualified.
	MUD PUMP



	7.2
	MUD TANKS

Minimum180 m3 and must meet the following minimum list of requirements:

a. Complete with pit agitators. 

b. Mud tanks to have positive sealing clean out gates.
c. Mud tanks must be equipped with suction line to pump, suction lines must have positive sealing suction valve, all active system mixing pumps must be able to deliver to every compartment in the active system 

d. Active mud system must be equipped with venturi or cyclone mixer, minimum 1 (one) 5” X 6” mixing pump manifolded to rig pump manifold and able to transfer fluids or to mix.

e. LP mud system must be capable of delivering fluid from the active mud system to storage tanks, mud pump, wellhead or cement unit

f. Mixing pump delivery system, piping & plumbing must meet manufacturers recommended specifications for optimum performance

g. Flow connector system between tanks must be positive sealing. 

h. All compartments fitted with ladders, covered with grating with hinged man entry opening for access to ladder.

i. Tanks fitted with stairs one end & ladder on opposite end

j. Sealing connector system between tanks must be positive sealing

k. Main tank minimum 40m3 capacity & transportable on pump carrier or oilfield skid mounted on bed loadable skids

l. Complete mud tank system must be fitted with sufficient explosion proof electric lighting for safe 24hr operation
	

	7.3
	 SHALE SHAKER

a. Mounted on main mud tank

b. Minimum screen 3’ wide x 4’ length

Screen mesh: 120 (provide by contractor)
	

	7.4
	MUD MIXING SYSTEM 

a. 1 cyclone or venturi Minimum 5X6 feed pump w/11” impellor driven by electric motor. The mixing system must be installed as per the manufacturers recommendations in order to insure maximum efficiency and rated performance 

b. Manifolded to transfer tank fluids 

c. Part of main tank system
	

	7.5
	PIT LEVEL INDICATOR

a. Digital pit level indicators with remote read outs
	

	7.6
	Bell nipple and mud ditch

1 set of mud umbrella and mud ditch should be installed to guide fluid through mud ditch into flow divider on NO1 tank.
	

	7.7
	Charge pump

Min 1 charge pump (sand pump) with switch maximum flow rate at least 4 m3/hr with fixed entrance in bell nipple
	

	7.8
	N/A
	

	7.9
	MUD PIT AGITATORS

Minimum 10 HP-drive motors, one in each compartment.
	

	7.10
	MUD FLOW TROUGHS

a. Equipped with settling system
	a. 

	7.11
	STANDPIPE

a. Minimum 5000psi WP

b. Minimum 2" nominal ID
	a. 

	7.12
	MUD GAS SEPARATOR H2S SERVICE 

H2S Service, Poor boy or standalone enclosed type. Poor boy type located in mud tanks must be situated in a separate compartment equipped with positive seal isolation valves fill up and fluid level control. This compartment cannot be included as part of the mud tank active system volume. Either type must be equipped with positive sealing “man hole” inspection covers for routine inspection and maintenance.
	

	7.13
	KELLY (ROTARY) HOSE

a. Minimum 5000psi WP

b. Minimum 2" ID

c. Minimum requirement 1 use, long enough 

d. Fitted with API figure 1502 male/female unions
	

	7.14
	SWIVEL 

a.
Manufacturer:

b.
Model:

c.
Maximum Load capacity- minimum 150 MT and compatible to mast and rotary table.

d.
Working Pressure - minimum 5000psi

e.
Year/date of made:

f.
Quantities: Minimum one.

Bidder failed to meet the minimum requirement will be directly disqualified.
	

	7.15
	WATER TANK 

Company suggests 80 m3 rig water storage, 5m3 brake water storage, 12 m3 potable water storage. 

a. Rig water storage minimum 80 m3, closed horizontal, bed loadable skid mounted with transfer circulating pumps  

b. Brake water tank if required, c/w after coolers & circulating system 

c. Potable water storage for rig site accommodations c/w circulating system 
	

	8
	BOP GENERAL INFORMATION

	8.1
	ANNULAR PREVENTER

a. Rated working pressure: 13-5/8” x 5,000 psi working pressure bag type preventer
b. Nominal size: 13-5/8”
c. Manufacturer:

d. Type:

e. Height (m):

f. Year/date of made: 
	

	8.2
	RAM TYPE PREVENTERS 

a. Rated working pressure: min 5000psi
b. Nominal size: 13-5/8”
c. Manufacturer:

d. Type:

e. Height of each (blind + pipe ram+ annular): 

f. Year/date of made: 

Must include blind + pipe ram 
	

	8.3
	BOP SKID / TOOL BOX

a. Fitted with BOP test flange & pressure valve test receptacle 

b. Fitted with Test Plug for BOP. 

c. Skidded & balanced for bed loading and of sufficient capacity to transport contractors’ sub, flange, spool, rotary tongs etc. on rig moves
	

	8.4
	CHOKE MANIFOLD
Component type 5,000psi WP, rigged to accept 2 automatic/manual choke, c/w gauges, provision for 3 sensors. Able to isolate chokes and pressure gauges for repair and replacement during operation. Able to flow through any choke to mud gas separator or to flare pit or any of 3 separate lines to tanks or flare pit. All gauges must be in small increments, easy to read faceplates, consistent sizing & type of pressure sensor is a requirement all gauges throughout the system must also be fully compatible. COMPANY reserve the option to modify the manifold as necessary
	

	8.5
	AUTOMATIC / MANUAL ADJUSTABLE CHOKE

1 each AUTOMATIC / MANUAL ADJUSTABLE CHOKE
Must meet minimum requirements consistent with choke manifold sizing and pressure rating
	

	8.6
	ACCUMULATOR UNIT RIG CARRIER MOUNTED or SKID MOUNTED
Minimum working pressure 3000psi, minimum usable volume contained in nitrogen activated storage bottles, each storage bottle must be equipped with isolation valve and pressure charge up/bleed off assembly. Pressured by rig hydraulic system, sufficient fluid storage volume included in rig hydraulic tank minimum 1 pneumatically operated charge pump, failure and pressure drop warning alarms local & remote, pressure regular & related valves, minimum 4 station 3-way control valves (open, neutral, close) on unit  

NOTE: Rigs not equipped with carrier mounted accumulator systems must have remote control panel at drillers station
	

	8.7
	PNUEMATIC PUMPS
Minimum one set
	

	8.8
	ALARM TYPES

a. Warning light

b. Siren, horn or klaxon
	

	8.9
	KILL LINE 

Minimum 50,00psi WP, flexible hose must be fitted with API figure 1502 male/female unions
	

	8.10
	KILL MANIFOLD 

Component type 5,000psi WP, equipped with enough gate valves and figure 1502 5K union to kill well by down tubing or reverse circulation or flow the well by switch the valves. Bidder shall describe the valves of the device and parameters.
Note：Shall have gate valves suits for connect with 2” 1502 5k pipe line from mud pump and outlet can connect 2” 1502 high pressure hose. Or shall be connectable with contractor’s lines.
	

	8.11
	N/A
	

	8.12
	DRILLING SPOOL AND VALVES

a) 1 drilling spool 13-5/8” X 5,000 psi WP with 2 flanged outlets (minimal 4-1/16” x 5000 psi WP), height
b) 2 flanged gate valves (minimum 4-1/16” x 5,000 psi WP)

c) 2 flanged HCR valve (minimum 4-1/16” x 5,000 psi WP)
	

	8.13
	N/A
	

	8.14
	FLARE LINE 

minimum 100 meters


	

	9
	AUXILIARY AND COMMUNICATION EQUIPMENT
	

	9.1
	AIR COMPRESSORS

a.
Minimum 2 each must be capable of supplying normal rig air supply; 

b.
An air dryer system must be included in the main air supply system to insure clean dry air. 

c.
Air storage vessels must be inspected and certified by a Company approved internationally recognized governing body
	

	10
	AUXILLIARY DEVICE 
	

	10.1
	PIPE RACKS

minimum 2 matching sets of racks compatible to catwalk.
	

	10.2
	CATWALK

a. Equipped with stairs at both ends, lay down trough

b. Removable lay down post

c. Equipped with minimum 40’ length

d. Must be adequately illuminated for safe 24hr operation
	

	10.3
	RAMP

e. Equipped with guide railings both sides

f. Must be adequately illuminated for safe 24hr operation
	

	10.4
	RIG STAIRS

a. All rig stairs must be in as good condition and equipped with hand railings

b. All rig stairs must be adequately illuminated for safe 24hr operation

c. Adjustable for level positioning
	

	10.5
	HAND RAILINGS

All rig hand railing must be of sufficient height and strength, equipped with kick boards and in as new condition
	

	10.6
	TUBING / DRILL PIPE RACKING PLATFORM 

a. Capable of racking & supporting 3000 meters 3-1/2” drill pipe, 2-7/8” and 3-1/2” tubing and BHA 

b. No spill type
	

	11
	SAFETY AND FIRE FIGHTING EQUIPMENT
	

	11.1
	GAS DETECTION / ALARM SYSTEM

a. Minimum 2 sensors with alarm,multigas 4x4 Flammable(H2S,O2,SO2,CH4)detector.
b. Minimum 4 fixed monitoring detector and alarm system with bacon light for detection of H2S (Cellar, drill floor, shale shaker and mud tank)
	Confirmed

	12
	HANDLINGANDTRANSPORTATIONEQUIPMENT
	

	12.1
	WHEELED ARTICULATING LOADER

Equivalent to Caterpillar 966F equipped with quick attach bucket and standard size pallet forks. Minimal load: 5 tons. Inspected and certified to a Company approved international oilfield industry safety standard. Must be equipped with HF or VHF radio.
	

	12.2
	Cameras
Surveillance cameras will be installed on the workover rig at:  

1-Rig floor 

2-Monky Board  

3-Cat walk and draw works area 

4-Well pad main entrance  
	

	12.3
	20’Container with shelves:

Storage container with shelves minim 20’ for storage the company equipment such as: completion equipment, wellhead spare parts, hydraulic pumps and all others equipment belong to company
	

	13
	CAMPPLAN
	

	13.1
	Camp is not a unitized side by side type. Maximum accommodation per room 4 persons, all rooms must be equipped with overhead and night lights, air conditioning, fire/smoke alarms emergency night lighting, fire extinguishers, and lockable lockers for each occupant. The camp water system must include a water filtration and chlorine treatment system. Equipped with 2 power generators each capable of handling the complete camp electrical requirements.
	

	13.2
	a. 1 potable water tank 

b. 1 unit: Dinning Hall

c. 2 warehouse (1 C/W air condition)

d. 3 tool house
e. 1 unit meeting Room 
f. 1 unit of clinic
g. 6 units 4 beds room
h. 3 units 2 beds room 
i. 4 units 8 beds room
j. 1 unit Power Distribution Cabinet
Please specify for item a – n as accurate as possible. Put the necessary remarks, if applicable. Please specify as accurate as possible. Put the necessary remarks, if applicable. 
	


(In Bidder's Letterhead)

ATTACHMENT 2-C DEVIATIONS/EXCEPTIONS BY BIDDER (UNPRICED)

(To be submitted in Technical Bid Proposal submission only without revealing any cost impact)

	Serial No.
	ITB Reference
	Clause/Article reference
	Deviations/Exceptions
	Cost Impact

(Yes/ No)
	Remark

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


(In Bidder's Letterhead)

ATTACHMENT 2-D LITIGATION DECLARATION 

[Indicate date of submission of the Bid]
Bidder’s name: [indicate Bidder’s name]

The Bidder hereby declares the following:

	1)
	The Bidder is currently involved in litigation since inception along with implication.
	Yes / No

	
	(If the answer to the above is “Yes”, please provide the relevant details in a separate sheet of paper)


	

	2)
	In the event the Bidder consists of a joint-venture, partnership, consortium or any other form of joint endeavor, any or all of the members of such joint-venture, partnership, consortium or any other form of joint endeavor are currently involved in litigation since inception along with implication.
	Yes / No

	
	(If the answer to the above is “Yes”, please provide the relevant details in a separate sheet of paper)


	

	3)
	The Bidder has been involved in the last 5 years in litigation since inception along with implication.
	Yes / No

	
	(If the answer to the above is “Yes”, please provide the relevant details in a separate sheet of paper)


	

	4)
	In the event the Bidder consists of a joint-venture, partnership, consortium or any other form of joint endeavour, any or all of the members of such joint-venture, partnership, consortium or any other form of joint endeavour have been involved in the past 5 years in litigation since inception along with implication.
	Yes / No

	
	(If the answer to the above is “Yes”, please provide the relevant details in a separate sheet of paper)
	


[Indicate Bidder’s name]
____________________________

Name: [indicate name of signatory]
Title: [indicate title of signatory]

(In Bidder's Letterhead)

ATTACHMENT 2-E CONFIDENTIALITY AND SECRECY DECLARATION

Pursuant to the provisions of the CONTRACT and BID documents (Invitation to BID dated ___________) between CNPC Bohai Drilling Engineering Company Limited- Iraq Branch (referred to as Tenderee), and _________________ (referred to as Bidder), the Bidder hereby declares and agrees that:
1.   All documents delivered to Bidder shall be handled confidentially and shall be used only for the purpose of preparing the Bid. Such documents shall not be duplicated or disclosed to others unless explicitly for the purpose of formulating the Bid in response to this invitation to Bid;

2.   The prices in the Bid have been arrived at independently, without consultation, communication, agreement or understanding for the purpose of restricting competition, as to any matter relating to such prices, with any other bidders or with any competitors;

3.   Unless otherwise required by law, the prices which have been quoted in the Bid have not knowingly been disclosed by Bidder, directly or indirectly, to any other bidders or competitors, nor will they be so disclosed;

4.     No attempt has been made or will be made by Bidder to induce any other person or company to submit or not to submit a Bid for the purpose of restricting competition; and Bidder has adhered to the highest standards of business ethics and, in particular, has established precautions to prevent any of its officers, employees, or agents from making, receiving or offering substantial gifts, entertainment, payment, loans, or other considerations which may influence individuals in respect of this invitation to Bid.
5.     This Declaration shall be construed under and governed by the law stipulated in the CONTRACT.

Signed:  ________________________________

Name:   ________________________________ 
Position held: ___________________________
On behalf of BIDDER: ___________________
Address: _______________________________  

 (In Bidder's Letterhead)

ATTACHMENT 3-A COMMERCIAL PROPOSAL FORM

1. Iraq 750HP Workover Rig Service Quotation
	No.
	Item
	Unit Price (USD)

	1
	Workover rig mobilization fee
	

	2
	Workover rig service daily rate
	

	3
	Annual workover rig service fee
	


Note: 
a) A withholding tax of Seven Percent (7%) shall be deducted from each service invoice in accordance with Iraqi tax law. 

b) The Contractor shall be responsible for customs clearance and mobilization of the workover rig to the location designated by the Company. The Company shall bear the mobilization fee and shall pay the first mobilization installment of USD 150,000 within 30 days after the workover rig commences shipment, and the remaining mobilization fee within 30 working days after the equipment arrives at the location designated by the Company.

c) If the Company requires additional equipment, the Company shall be responsible for the mobilization work and all related mobilization costs.
d) The workover rig service fee shall accrue from the date the first well spuds and continue on a calendar-day basis at the Daily Rate (Item 2). Settlement shall be made on a calendar-quarter basis. Contractor shall submit a timesheet and invoice for each quarter, and Company shall make payment within ninety (90) days upon receipt of the invoice. The Annual Service Fee (Item 3) is provided for budgetary reference only and shall not be used in any settlement calculation, nor shall it be charged in addition to or in duplication with the Daily Rate.

e) Company will be responsible for providing equipment maintenance and servicing, spare parts and replacements, lubricants, and all types of oils.
(In Bidder's Letterhead)

ATTACHMENT 3-B  DEVIATIONS/EXCEPTIONS BY BIDDER (WITH PRICE)

(To be submitted in Commercial Bid Proposal submission only with price)
	Serial No.
	ITB Reference
	Clause/Article reference
	Deviations/Exceptions
	Cost Impact

(List out the detail price)
	Remark
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